{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"charts":0,"images":2,"macros":0,"external_links":1,"defined_names":14,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":16,"n_cols":11,"rows_kept":16,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[]
[null,null,null,"G8KHW Path loss Calculator "]
[]
[null,433.92,"<- frequency (in MHz)",null,null,1,"<- TX power (watts)",null,null,10,"<- TX ant gain (dBi)"]
[null,200,"<- distance (in Km)",null,null,0,"<= TX power (dbW)",null,null,-3,"<-Rx ant. Gain (dBi)"]
[]
[null,0.6913716814159292,"<= wavelength",null,null,2.4,"<- RX bandwidth (Khz)"]
[null,-131.21056545634733,"<= pathloss (db)",null,null,100,"<- Sky Noise (deg K) – read off from fig. below"]
[{"$nulls":5},93,"<- Noise Figure (deg K) – read off from fig. below"]
[{"$nulls":6}," "]
[null,"Line of Sight (LoS) calculator"]
[null,30,"<-height (km)",null,null," "]
[null,619.1930232165088,"<=LoS distance (km)",null,null,-171.94352362879383,"<= receiver noise (dbW)"]
[]
[]
[{"$nulls":8},47.7329581724465,"<= overall margin (db)"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}